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	Dane samochodu

	

	

	Marka:
	A
	Nr identyfikacyjny samochodu:
	WAUZZZ4BX2N064160
	Kod kraju:
	DEU
	
	
	
	

	Rok modelowy:
	2002
	Opis:
	A6 Ava. quat.2.7 V6184 A5
	Region:
	136
	
	
	
	

	Typ handlowy:
	4B507Z
	Data produkcji:
	2001-11-15
	Nr partnera:
	26107
	
	
	
	

	MKB:
	ARE
	Data wydania samochodu:
	2001-11-23
	Leasing:
	
	
	
	
	

	GKB:
	FAX
	Nr homologacji typu:
	
	
	
	
	
	
	

	Kolor wyposażenia

	Typ
	Kod barwny
	Nr lakieru (nr KD lakieru)
	Opis

	z zewnątrz (nadwozie/dach)
	4Z/4Z
	LZ9W 
	Ebony Black, pearl effect/Ebony Black, pearl effect

	wewnątrz
	LF
	
	light grey/grey-light grey/light grey/ light grey


	Numery PR
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	Pochodzenie [image: image8.png]



	Grupa [image: image9.png]



	Opis [image: image10.png]




	
	0DS
	L
	AED
	installation differentiation for build status of vehicle class 4B0 (AUDI)

	
	0F2
	L
	KRS
	fuel system for carburetor gasoline engine

	
	0G7
	L
	GES
	Tiptronic

	
	0GE
	L
	AGM
	emissions concept EU 3

	
	0JL
	L
	GKV
	weight category front axle weight range 11

	
	0LW
	L
	SIZ
	special plates/stickers/ safety certificates for Germany

	
	0N6
	L
	HIA
	rear axle with reduced tread

	
	0ST
	L
	SAU
	labels/plates in German and French

	
	0VC
	L
	BTA
	information kit in German

	
	0W1
	L
	AKZ
	label for central electric German-speaking countries

	
	0YS
	L
	GKH
	weight category rear axle weight range 16

	
	1BE
	E
	DAE
	sports suspension/shock absorption

	
	1C1
	L
	FRO
	antifreeze up to -25 degree celsius tolerance up to -30 degree C

	
	1D2
	P
	AHV
	removable and lockable towing attachment

	
	1EX
	L
	TYP
	special identification plate for EC

	
	1G3
	L
	RER
	alloy spare wheel with original equipment tires

	
	1KD
	L
	BAH
	disc brakes, rear

	
	1LG
	L
	BAV
	disc brakes, front

	
	1MU
	P
	LRA
	leather trimmed sports steering wheel for airbag system with Tiptronic

	
	1N1
	L
	LEN
	power steering

	
	1PC
	L
	ABR
	wheel bolts with anti-theft protection (unlockable)

	
	1SA
	L
	TWU
	without additional engine guard

	
	1T3
	L
	VBK
	First aid kit with warning triangle

	
	1VH
	L
	TWL
	installation parts for six-cylinder engine

	
	1WD
	L
	GFW
	transmission shaft for tripod joints

	
	1X1
	L
	ATA
	four wheel drive

	
	1YD
	L
	GFH
	transmission shafts for rear axle diameter 108

	
	1Z2
	L
	KRM
	increase in initial standard fuel filling

	
	2A4
	P
	UEA
	delivery equipment for shipment (transitcoating) with thick seat cover

	
	2B5
	L
	GRD
	additional exterior noise suppression

	
	2C5
	L
	LSS
	axial and vertical adjustable steering column

	
	2G1
	L
	EBB
	insert for the filling up of unleaded fuel

	
	2K6
	L
	SFS
	reinforced bumpers

	
	2T0
	L
	DAT
	without double-sized standard (DIN)

	
	2Z0
	E
	TYZ
	deletion of model designation

	
	3B0
	L
	ZKV
	without additional child seat anchor

	
	3C7
	L
	SHM
	3-point seat belt for center rear seat

	
	3CB
	L
	TRW
	removable net partition

	
	3DF
	E
	ZBR
	winter tires 205/55 R 16 H with alloy wheel 6J x 16, offset 40 A6 design

	
	3FA
	L
	DEI
	without roof insert (standard roof)

	
	3GD
	L
	LBH
	plane rear cargo area

	
	3HA
	L
	LTU
	without leather parts scope

	
	3NZ
	L
	HIS
	rear seat bench unsplit, backrest split folding

	
	3PF
	L
	SIE
	electric height adjustment for both front seats

	
	3Q6
	L
	KOH
	three rear headrests

	
	3S1
	E
	DAR
	bright roof rails

	
	3V0
	L
	KSB
	without child bench seat

	
	3X1
	E
	DLS
	load-through provision with ski bag

	
	3Y0
	L
	SSR
	without roll-up sun screen

	
	4E0
	L
	SDH
	tailgate/trunk lid unlocking from outside

	
	4A3
	P
	SIH
	seat heater for front seats separately controlled

	
	4GH
	L
	WSS
	windshield tinted with windshield sunshield

	
	4K4
	L
	TKV
	radio remote controlled central locking

	
	4KC
	L
	SSH
	side and rear windows tinted

	
	4L2
	L
	IRS
	dipping breakaway inside rear view mirror

	
	4N0
	L
	INT
	standard dashboard

	
	4UE
	L
	AIB
	airbag f. driver a. front seat passenger

	
	4W0
	L
	KBO
	without cassette and CD storage unit

	
	4X3
	L
	SAB
	side airbag front with curtain airbag

	
	4ZB
	L
	ZIE
	bright moldings

	
	5A5
	L
	GRV
	trunk lining, with stowage trays

	
	5C0
	L
	KSA
	without special body measures

	
	5D1
	L
	TRF
	carrier frequency 433.92 MHz

	
	5K1
	L
	LAC
	paint preservative (wax)

	
	5RU
	L
	ASR
	outer right rear view mirror: convex (large viewing field)

	
	5SL
	L
	ASL
	outer left rear view mirror: non-spherical

	
	5TZ
	E
	EIH
	decorative inserts, gray birch vein

	
	6FB
	L
	BBO
	body-colored outer rear view mirror housings

	
	6M1
	L
	GPS
	tie down straps

	
	6PC
	P
	HBV
	leatherette hand brake lever handle

	
	6Q2
	P
	SAG
	leather gearshift knob/handle

	
	6R0
	L
	SHV
	selector lever cover

	
	6SS
	L
	KBB
	luggage compartment floor covering

	
	6U0
	L
	ZTD
	without additional seals outside

	
	6V1
	L
	HEB
	rear trim panel (ECE)

	
	6W5
	L
	KZV
	front license plate bracket

	
	6XD
	L
	ASE
	outer rear view mirrors: powered, heated

	
	7E0
	L
	WSA
	w/o heat accumulator/auxiliary heating

	
	7A0
	L
	CDW
	without CD changer/CD player

	
	7AA
	L
	EDW
	electronic vehicle immobilization device

	
	7K0
	L
	RDK
	without tire pressure warning light

	
	7M1
	L
	EIL
	scuff plates in door apertures with metal inserts

	
	7P1
	P
	LOR
	power adjustable lumbar support in frontseats

	
	7Q9
	P
	NAV
	navigation system

	
	7QB
	P
	CDR
	CD ROM (Germany)

	
	7X1
	P
	EPH
	Park distance control

	
	8ED
	P
	HSW
	bi-functional headlight with gas discharge lamp, for driving on the right

	
	8GL
	L
	GEN
	alternator 120A

	
	8K0
	L
	FLS
	without special low beam mode

	
	8N4
	L
	SWS
	windshield wiper intermittent control with potentiometer (four speeds)

	
	8Q3
	P
	LWR
	automatic headlight-range adjustment dynamic (self-adjusting while driving)

	
	8T0
	L
	GRA
	without cruise control system (CCS)

	
	8TC
	L
	NEL
	rear fog light for driving on the right

	
	8UD
	E
	RAO
	radio "concert"

	
	8X1
	P
	SWR
	headlight washer system

	
	8Z5
	L
	MKU
	engine cooling system, type 1

	
	9AK
	L
	HKA
	"Climatronic" with impact pressure control free of cfc

	
	9B0
	L
	TPG
	without telepay device

	
	9M0
	L
	ZUH
	without auxiliary/parking heater

	
	9NX
	L
	FAS
	without electronic logbook

	
	9P0
	L
	SGK
	without seat belt warning light

	
	9Q2
	P
	MFA
	multi-function indicator/on-board computer with check control

	
	9VD
	P
	LSE
	speaker (active)

	
	9ZF
	E
	VTV
	preparation for cellular phone with hands-free speaking system

	
	1E1
	L
	AKB
	activated carbon canister

	
	5E2
	L
	SAA
	sill top with door cover

	
	6E3
	E
	MAS
	center armrest front

	
	A00
	L
	SAH
	no self-collection

	
	A8S
	I
	AUS
	standard equipment

	
	B0A
	L
	BLB
	component parts set without country-specific design requirement

	
	B01
	L
	TPL
	type approval Germany

	
	C9K
	L
	RAD
	alloy wheels 7J x 16 5-arm rotor style, offset 45

	
	C18
	E
	COC
	operating permit, alteration 18

	
	E0A
	L
	AAU
	no special edition

	
	F0A
	L
	FZS
	no special purpose vehicle, standard equipment

	
	FA0
	L
	SVO
	control of standard production

	
	FC0
	L
	IND
	without customized installation

	
	FQ0
	L
	QGM
	standard production wheels

	
	G0Q
	I
	GSP
	five-speed automatic transmission for four-wheel drive vehicle

	
	H3R
	L
	REI
	tires 215/55 R 16 93Y

	
	J0L
	L
	BAT
	battery 340 A (70 Ah)

	
	K8D
	I
	KAR
	Station Wagon Variant/Avant

	
	L0L
	L
	LEA
	left-hand drive vehicle

	
	MK5
	L
	MOT
	6-cyl. gasoline engine 2.7 L/184 kW 30V base engine is T7Z

	
	N1H
	P
	SIB
	leather seat covering

	
	NT0
	L
	TSP
	transit coating (type 1)

	
	P18
	G
	
	leather-covered sports steering wheel, three spokes, switching functions

	
	PAA
	G
	
	trailer towing hitch

	
	PLD
	G
	
	Buffalino leather

	
	PNH
	G
	
	navigation system (BNS 4.1)

	
	PPA
	G
	
	Acoustic Parking System (APS)

	
	PSV
	G
	
	seat heating for front seats

	
	PX4
	G
	
	xenon Plus headlights

	
	Q1D
	P
	VOS
	sports front seats

	
	QA0
	L
	KIS
	without child seat

	
	QH0
	L
	SPR
	without voice control

	
	QV0
	L
	TVE
	w/o TV reception/digital radio reception

	
	RLA
	G
	
	active speaker system

	
	T7Z
	I
	GMO
	6-cylinder gasoline engine 2.7 L unit 078.8

	
	U2B
	L
	INS
	instrument insert with km/h speedometer,radio-controlled clock, tachometer, tripodometer and additional instruments

	
	V0A
	L
	REL
	tires w/o specification of tire brand

	
	VC0
	L
	GRT
	w/o remote-controlled garage door opener

	
	VX0
	L
	SPA
	without hands-free system

	
	VY0
	L
	GAS
	without danger alarm system

	
	WS1
	G
	
	front sports seats

	
	X0A
	G
	
	national sales program Germany
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